Argument1

Evidence3

Evidence2

Evidence1

Justification

Clime

Arg1 / strategy

ECU will run a basic test each time the ON brake signal is captured, and determine if any errors are present.

ECU will turn on an ABS error light on the driver's console if an error occurs in the system.

ECU will run a system diagnostic test sequence at ignition and determine if any errors are present in the system.

ABS is safe in current context

Controls to detect ABS system failures is effectively.